# MHT-P80A flash

1. Connect the printer USB cable to the computer and keep it in the off state.

2. First, press and hold the printer's paper output button, and then press and hold the printer's power button. After powering on, immediately let go of the paper eject button.

3. Note: If the operation is successful, there will be no sound when the machine is turned on. If the operation fails, there will be a sound when the machine is turned on. Failed to re-operate

4. Operate the flashing tool

5. Flashing tool





